;
;   TivaWare USB CDC (serial) driver installation file.
;
;   Copyright (c) 2010 Texas Instruments Incorporated.  All rights reserved.
;

[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%MFGNAME%
CatalogFile.NTx86=usb_dev_chidcdc_x86.cat
CatalogFile.NTamd64=usb_dev_chidcdc_amd64.cat
LayoutFile=layout.inf
DriverVer=02/07/2014,2.1.0.12573

[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
%12%\usbser.sys=1

[Manufacturer]
%MFGNAME%=VirComDevice,NT,NTamd64

[DestinationDirs]
DefaultDestDir = 12

[VirComDevice.NT]
;
; This entry is for the composite hid/serial device usb_dev_chidcdc.  Notice
; that the value is MI_01 because the serial device is on interface 1.
;
%DESCRIPTION%=DriverInstall,USB\Vid_1CBE&Pid_0009&MI_01

[VirComDevice.NTamd64]
;
; This entry is for the composite hid/serial device usb_dev_chidcdc.  Notice
; that the value is MI_01 because the serial device is on interface 1.
;
%DESCRIPTION%=DriverInstall,USB\Vid_1CBE&Pid_0009&MI_01

[DriverInstall.NT]
Include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverInstall.NT.AddReg

[DriverInstall.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NT.Services]
AddService=usbser, 0x00000002, DriverServiceInst

[DriverServiceInst]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys

[Strings]
MFGNAME       = "Texas Instruments, Inc."
DISKNAME      = "TivaWare Composite Serial Device"
DESCRIPTION   = "TivaWare USB Serial Command Port"
SERVICE       = "TivaWare USB CDC serial port"
